# Static Call Graph for image ..\OBJ\STM32F030Demo.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Tue Nov 29 15:10:17 2022

### Maximum Stack Usage = 244 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ displayPageInformation ⇒ displayPDataSpec ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init

### Mutually Recursive functions

- HardFault_Handler ⇒ HardFault_Handler
- ADC1_COMP_IRQHandler ⇒ ADC1_COMP_IRQHandler

  ### Function Pointers

  - ADC1_COMP_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - CEC_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - DMA1_Channel2_3_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - DMA1_Channel4_5_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - EXTI0_1_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - EXTI2_3_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - EXTI4_15_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - HardFault_Handler from stm32f0xx_it.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - I2C1_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - I2C2_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - NMI_Handler from stm32f0xx_it.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - PendSV_Handler from stm32f0xx_it.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - RTC_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - Reset_Handler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - SVC_Handler from stm32f0xx_it.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - SysTick_Handler from stm32f0xx_it.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - SystemInit from system_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(.text)
  - TIM14_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TIM15_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TIM16_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TIM17_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TIM1_BRK_UP_TRG_COM_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TIM3_IRQHandler from delay.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - TS_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - USART1_IRQHandler from usart.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f0xx.o(.text) referenced from startup_stm32f0xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f0xx.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_lib_shutdown_fini (Thumb, 0 bytes, Stack size unknown bytes, entry12b.o(.ARM.Collect$$$$0000000E))
  [Calls]

  - >> __arm_fini_ (Weak Reference)

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000F))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$00000011))

  displaySettingPage (Thumb, 1060 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 156
  - Call Chain = displaySettingPage ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  - >> delay_ms
  - >> DisplayThirdLine
  - >> DisplaySecondLine
  - >> DisplayFourthLine
  - >> DisplayFirstLine
  [Called By]
  - >> main

  GetDatalength (Thumb, 138 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GetDatalength ⇒ __aeabi_fdiv
  [Calls]
  - >> __aeabi_fdiv
  [Called By]
  - >> displayHarmI
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayFreq
  - >> displayPData
  - >> displayHarmU
  - >> displayLC
  - >> displayMD
  - >> displayTempata
  - >> displayPowerData
  - >> displayUIData

  displayUIData (Thumb, 1170 bytes, Stack size 32 bytes, main.o(.text))
  [Stack]

  - Max Depth = 164
  - Call Chain = displayUIData ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLine
  - >> DisplaySecondLine
  - >> DisplayFourthLine
  - >> DisplayFirstLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayPowerData (Thumb, 2348 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = displayPowerData ⇒ OLED_5_Display ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> OLED_5_Display
  - >> __ARM_common_switch8
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayLoadRatio (Thumb, 364 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 124
  - Call Chain = displayLoadRatio ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPageInformation

  displayCtnum (Thumb, 664 bytes, Stack size 32 bytes, main.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = displayCtnum ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  - >> __ARM_common_switch8
  [Called By]
  - >> displayPageInformation

  JudgeMinus (Thumb, 132 bytes, Stack size 20 bytes, main.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = JudgeMinus
  [Called By]
  - >> displayPageInformation

  displayDIDO (Thumb, 32 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = displayDIDO ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPageInformation

  displayTempata (Thumb, 1012 bytes, Stack size 40 bytes, main.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = displayTempata ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLine
  - >> DisplaySecondLine
  - >> DisplayFourthLine
  - >> DisplayFirstLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayMD (Thumb, 258 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = displayMD ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLine
  - >> DisplayFourthLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayLC (Thumb, 258 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = displayLC ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLine
  - >> DisplayFourthLineSpec
  - >> DisplayFourthLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayHarmU (Thumb, 258 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = displayHarmU ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLine
  - >> DisplayFourthLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayPData (Thumb, 1232 bytes, Stack size 40 bytes, main.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = displayPData ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLine
  - >> DisplaySecondLine
  - >> DisplayFourthLine
  - >> DisplayFirstLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayFreq (Thumb, 258 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = displayFreq ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLine
  - >> DisplayFourthLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayPDataSpecVA (Thumb, 1120 bytes, Stack size 40 bytes, main.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = displayPDataSpecVA ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLineSpec
  - >> DisplayThirdLine
  - >> DisplaySecondLine
  - >> DisplayFourthLineSpec2
  - >> DisplayFourthLine
  - >> DisplayFirstLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayPDataSpec (Thumb, 898 bytes, Stack size 40 bytes, main.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = displayPDataSpec ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplayThirdLine
  - >> DisplaySecondLineSpec
  - >> DisplaySecondLine
  - >> DisplayFourthLine
  - >> DisplayFirstLineSpec
  - >> DisplayFirstLine
  - >> GetDatalength
  - >> __aeabi_idivmod
  [Called By]
  - >> displayPageInformation

  displayPageInformation (Thumb, 3240 bytes, Stack size 72 bytes, main.o(.text))
  [Stack]

  - Max Depth = 244
  - Call Chain = displayPageInformation ⇒ displayPDataSpec ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  - >> __aeabi_fdiv
  - >> __ARM_common_switch8
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayFreq
  - >> displayPData
  - >> displayHarmU
  - >> displayLC
  - >> displayMD
  - >> displayTempata
  - >> displayDIDO
  - >> JudgeMinus
  - >> displayCtnum
  - >> displayLoadRatio
  - >> displayPowerData
  - >> displayUIData
  [Called By]
  - >> main

  main (Thumb, 94 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 244
  - Call Chain = main ⇒ displayPageInformation ⇒ displayPDataSpec ⇒ DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> requestData
  - >> keyHandle
  - >> init_ht16c23
  - >> delay_ms
  - >> delay_init
  - >> USART1_Init
  - >> TIM3_Init
  - >> SystemInit
  - >> MX_GPIO_Init
  - >> LEDInit
  - >> LEDHandle
  - >> KEY_Init
  - >> ExistRXInformation
  - >> displayPageInformation
  - >> displaySettingPage
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  displayHarmI (Thumb, 288 bytes, Stack size 16 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> DisplaySecondLine
  - >> DisplayFirstLine
  - >> GetDatalength
  - >> __aeabi_idivmod

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f0xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 0 bytes, system_stm32f0xx.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ RCC_PLLConfig
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - startup_stm32f0xx.o(.text)

  SystemCoreClockUpdate (Thumb, 106 bytes, Stack size 16 bytes, system_stm32f0xx.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))

  ADC1_COMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Calls]

  - >> ADC1_COMP_IRQHandler
  [Called By]
  - >> ADC1_COMP_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f0xx.o(RESET)

  CEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  DMA1_Channel2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  DMA1_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  EXTI0_1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  EXTI2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  EXTI4_15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM1_BRK_UP_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f0xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f0xx.o(RESET)

  TIM3_Init (Thumb, 86 bytes, Stack size 24 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = TIM3_Init ⇒ NVIC_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_ClearITPendingBit
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> main

  delay_ms (Thumb, 46 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> HAL_TIM_PeriodElapsedCallback
  - >> main
  - >> displaySettingPage

  HAL_TIM_PeriodElapsedCallback (Thumb, 208 bytes, Stack size 24 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_PeriodElapsedCallback
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> delay_ms
  [Called By]
  - >> TIM3_IRQHandler

  TIM3_IRQHandler (Thumb, 30 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = TIM3_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback
  [Calls]
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  - >> HAL_TIM_PeriodElapsedCallback
  [Address Reference Count : 1]
  - startup_stm32f0xx.o(RESET)

  delay_init (Thumb, 36 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = delay_init ⇒ __aeabi_uidivmod
  [Calls]
  - >> SysTick_CLKSourceConfig
  - >> __aeabi_uidivmod
  [Called By]
  - >> main

  delay_us (Thumb, 46 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_Send_Byte

  MX_GPIO_Init (Thumb, 44 bytes, Stack size 16 bytes, gpio.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = MX_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHBPeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> IIC_Init
  - >> main

  O_GPIO_Init (Thumb, 28 bytes, Stack size 16 bytes, gpio.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  [Called By]
  - >> SDA_OUT

  I_GPIO_Init (Thumb, 26 bytes, Stack size 16 bytes, gpio.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = I_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  [Called By]
  - >> SDA_IN

  ht16c23_clear (Thumb, 60 bytes, Stack size 8 bytes, ht16c23.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = ht16c23_clear ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_Send_Byte
  [Called By]
  - >> keyHandle
  - >> init_ht16c23

  I2CWriteSingle (Thumb, 46 bytes, Stack size 16 bytes, ht16c23.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = I2CWriteSingle ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_Send_Byte
  [Called By]
  - >> init_ht16c23

  init_ht16c23 (Thumb, 52 bytes, Stack size 8 bytes, ht16c23.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = init_ht16c23 ⇒ I2CWriteSingle ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_Init
  - >> I2CWriteSingle
  - >> ht16c23_clear
  [Called By]
  - >> main

  ht16c23_write_one_byte2ram (Thumb, 56 bytes, Stack size 16 bytes, ht16c23.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_Send_Byte
  [Called By]
  - >> OLED_5_DisplaySpec
  - >> OLED_5_Display
  - >> DisplayThirdLineSpec
  - >> DisplayThirdLine
  - >> DisplaySecondLineSpec
  - >> DisplaySecondLine
  - >> DisplayFourthLineSpec2
  - >> DisplayFourthLineSpec
  - >> DisplayFourthLine
  - >> DisplayFirstLineSpec
  - >> DisplayFirstLine
  - >> displayPageInformation
  - >> displayDIDO
  - >> displayCtnum
  - >> displayLoadRatio
  - >> displayPowerData
  - >> displaySettingPage

  KEY_Init (Thumb, 64 bytes, Stack size 16 bytes, key.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = KEY_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHBPeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  keyHandle (Thumb, 578 bytes, Stack size 24 bytes, key.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = keyHandle ⇒ ht16c23_clear ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> USART1SendData
  - >> ht16c23_clear
  - >> __aeabi_memclr
  [Called By]
  - >> main

  SDA_OUT (Thumb, 8 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> O_GPIO_Init
  [Called By]
  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_Send_Byte

  SDA_IN (Thumb, 8 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = SDA_IN ⇒ I_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> I_GPIO_Init
  [Called By]
  - >> IIC_Wait_Ack

  IIC_Init (Thumb, 32 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = IIC_Init ⇒ MX_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> MX_GPIO_Init
  [Called By]
  - >> init_ht16c23

  IIC_Start (Thumb, 62 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = IIC_Start ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> SDA_OUT
  - >> delay_us
  [Called By]
  - >> I2CWriteSingle
  - >> ht16c23_clear
  - >> ht16c23_write_one_byte2ram

  IIC_Stop (Thumb, 62 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> SDA_OUT
  - >> delay_us
  [Called By]
  - >> IIC_Wait_Ack
  - >> I2CWriteSingle
  - >> ht16c23_clear
  - >> ht16c23_write_one_byte2ram

  IIC_Wait_Ack (Thumb, 88 bytes, Stack size 24 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> SDA_IN
  - >> IIC_Stop
  - >> GPIO_ReadInputDataBit
  - >> delay_us
  [Called By]
  - >> I2CWriteSingle
  - >> ht16c23_clear
  - >> ht16c23_write_one_byte2ram

  IIC_Ack (Thumb, 60 bytes, Stack size 16 bytes, myiic.o(.text), UNUSED)
  [Calls]

  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> SDA_OUT
  - >> delay_us

  IIC_NAck (Thumb, 60 bytes, Stack size 16 bytes, myiic.o(.text), UNUSED)
  [Calls]

  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> SDA_OUT
  - >> delay_us

  IIC_Send_Byte (Thumb, 100 bytes, Stack size 24 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = IIC_Send_Byte ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> SDA_OUT
  - >> delay_us
  [Called By]
  - >> I2CWriteSingle
  - >> ht16c23_clear
  - >> ht16c23_write_one_byte2ram

  OLED_5_Display (Thumb, 24 bytes, Stack size 8 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = OLED_5_Display ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPowerData

  OLED_5_DisplaySpec (Thumb, 24 bytes, Stack size 8 bytes, oled0561.o(.text), UNUSED)
  [Calls]

  - >> ht16c23_write_one_byte2ram

  DisplayFirstLine (Thumb, 382 bytes, Stack size 32 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = DisplayFirstLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayHarmI
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayPData
  - >> displayTempata
  - >> displayUIData
  - >> displaySettingPage

  DisplayFirstLineSpec (Thumb, 58 bytes, Stack size 16 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = DisplayFirstLineSpec ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPDataSpec

  DisplaySecondLine (Thumb, 382 bytes, Stack size 32 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = DisplaySecondLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayHarmI
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayPData
  - >> displayTempata
  - >> displayUIData
  - >> displaySettingPage

  DisplaySecondLineSpec (Thumb, 58 bytes, Stack size 16 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = DisplaySecondLineSpec ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPDataSpec

  DisplayThirdLine (Thumb, 384 bytes, Stack size 32 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = DisplayThirdLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayFreq
  - >> displayPData
  - >> displayHarmU
  - >> displayLC
  - >> displayMD
  - >> displayTempata
  - >> displayUIData
  - >> displaySettingPage

  DisplayThirdLineSpec (Thumb, 56 bytes, Stack size 16 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = DisplayThirdLineSpec ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPDataSpecVA

  DisplayFourthLine (Thumb, 380 bytes, Stack size 32 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = DisplayFourthLine ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayFreq
  - >> displayPData
  - >> displayHarmU
  - >> displayLC
  - >> displayMD
  - >> displayTempata
  - >> displayUIData
  - >> displaySettingPage

  DisplayFourthLineSpec (Thumb, 58 bytes, Stack size 16 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = DisplayFourthLineSpec ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayLC

  DisplayFourthLineSpec2 (Thumb, 62 bytes, Stack size 16 bytes, oled0561.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = DisplayFourthLineSpec2 ⇒ ht16c23_write_one_byte2ram ⇒ IIC_Wait_Ack ⇒ IIC_Stop ⇒ SDA_OUT ⇒ O_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> ht16c23_write_one_byte2ram
  [Called By]
  - >> displayPDataSpecVA

  USART1_Init (Thumb, 198 bytes, Stack size 56 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 140
  - Call Chain = USART1_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_ClearFlag
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> RCC_AHBPeriphClockCmd
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> main

  USART1_IRQHandler (Thumb, 102 bytes, Stack size 16 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  - >> USART_GetFlagStatus
  - >> USART_ClearFlag
  [Address Reference Count : 1]
  - startup_stm32f0xx.o(RESET)

  USART1TxData (Thumb, 40 bytes, Stack size 16 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART1TxData
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Called By]
  - >> USART1SendData
  - >> requestData

  GetCRC16 (Thumb, 42 bytes, Stack size 16 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = GetCRC16
  [Called By]
  - >> USART1SendData
  - >> ExistRXInformation

  USART1SendData (Thumb, 118 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1SendData ⇒ GetCRC16
  [Calls]
  - >> GetCRC16
  - >> USART1TxData
  - >> __aeabi_memcpy
  [Called By]
  - >> keyHandle

  ExistRXInformation (Thumb, 116 bytes, Stack size 24 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = ExistRXInformation ⇒ GetCRC16
  [Calls]
  - >> GetCRC16
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  [Called By]
  - >> main

  requestData (Thumb, 60 bytes, Stack size 16 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = requestData ⇒ USART1TxData
  [Calls]
  - >> USART1TxData
  - >> __aeabi_memclr
  [Called By]
  - >> main

  LEDInit (Thumb, 40 bytes, Stack size 16 bytes, led.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LEDInit ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHBPeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  LEDHandle (Thumb, 106 bytes, Stack size 20 bytes, led.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LEDHandle
  [Called By]
  - >> main

  GPIO_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f0xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHBPeriphResetCmd

  GPIO_Init (Thumb, 112 bytes, Stack size 20 bytes, stm32f0xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> I_GPIO_Init
  - >> O_GPIO_Init
  - >> USART1_Init
  - >> MX_GPIO_Init
  - >> LEDInit
  - >> KEY_Init

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 28 bytes, Stack size 8 bytes, stm32f0xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text))
  [Called By]

  - >> IIC_Wait_Ack
  - >> HAL_TIM_PeriodElapsedCallback

  GPIO_ReadInputData (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text))
  [Called By]

  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_Send_Byte
  - >> IIC_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text))
  [Called By]

  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_Send_Byte

  GPIO_WriteBit (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f0xx_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> USART1_Init

  RCC_DeInit (Thumb, 78 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 50 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 50 bytes, Stack size 12 bytes, stm32f0xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_AdjustHSI14CalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_HSI14Cmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_HSI14ADCRequestCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_LSEDriveConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f0xx_rcc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_PLLConfig
  [Called By]
  - >> SetSysClock

  RCC_PLLCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_PREDIV1Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text))
  [Called By]

  - >> SetSysClock

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_PCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 38 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_CECCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_I2CCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_USARTCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 232 bytes, Stack size 24 bytes, stm32f0xx_rcc.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = RCC_GetClocksFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> USART_Init

  RCC_RTCCLKConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_AHBPeriphClockCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text))
  [Called By]

  - >> USART1_Init
  - >> MX_GPIO_Init
  - >> LEDInit
  - >> KEY_Init

  RCC_APB2PeriphClockCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text))
  [Called By]

  - >> USART1_Init

  RCC_APB1PeriphClockCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text))
  [Called By]

  - >> TIM3_Init

  RCC_AHBPeriphResetCmd (Thumb, 54 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> TIM_DeInit
  - >> USART_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> TIM_DeInit
  - >> USART_DeInit

  RCC_ITConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_rcc.o(.text), UNUSED)

  NVIC_Init (Thumb, 72 bytes, Stack size 12 bytes, stm32f0xx_misc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = NVIC_Init
  [Called By]
  - >> USART1_Init
  - >> TIM3_Init

  NVIC_SystemLPConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_misc.o(.text))
  [Called By]

  - >> delay_init

  USART_DeInit (Thumb, 54 bytes, Stack size 8 bytes, stm32f0xx_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 182 bytes, Stack size 48 bytes, stm32f0xx_usart.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> RCC_GetClocksFreq
  - >> __aeabi_uidivmod
  [Called By]
  - >> USART1_Init

  USART_StructInit (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 30 bytes, Stack size 8 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text))
  [Called By]

  - >> USART1_Init

  USART_DirectionModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_MSBFirstCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_DataInvCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_InvPinCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SWAPPinCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_ReceiverTimeOutCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SetReceiverTimeOut (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_STOPModeCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_StopModeWakeUpSourceConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_AutoBaudRateCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_AutoBaudRateConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_AutoBaudRateNewRequest (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text))
  [Called By]

  - >> USART1TxData

  USART_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_MuteModeCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_MuteModeWakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_AddressDetectionConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SetAutoRetryCount (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SetBlockLength (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_DECmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_DEPolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SetDEAssertionTime (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_SetDEDeassertionTime (Thumb, 34 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_DMACmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_DMAReceptionErrorConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_ITConfig (Thumb, 46 bytes, Stack size 8 bytes, stm32f0xx_usart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ITConfig
  [Called By]
  - >> USART1_Init

  USART_RequestCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_OverrunDetectionConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text))
  [Called By]

  - >> USART1TxData
  - >> USART1_IRQHandler

  USART_ClearFlag (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler
  - >> USART1_Init

  USART_GetITStatus (Thumb, 60 bytes, Stack size 12 bytes, stm32f0xx_usart.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ClearITPendingBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f0xx_usart.o(.text), UNUSED)

  TIM_DeInit (Thumb, 206 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  TIM_TimeBaseInit (Thumb, 88 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TimeBaseInit
  [Called By]
  - >> TIM3_Init

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_GetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_GetPrescaler (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text))
  [Called By]

  - >> TIM3_Init

  TIM_BDTRConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_BDTRStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_CtrlPWMOutputs (Thumb, 28 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC1Init (Thumb, 108 bytes, Stack size 16 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC2Init (Thumb, 118 bytes, Stack size 16 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC3Init (Thumb, 114 bytes, Stack size 12 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC4Init (Thumb, 82 bytes, Stack size 12 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OCStructInit (Thumb, 86 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectOCxM (Thumb, 74 bytes, Stack size 12 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ForcedOC1Config (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectOCREFClear (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 22 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 22 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 90 bytes, Stack size 16 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TI1_Config
  - >> TI2_Config
  - >> TI3_Config
  - >> TI4_Config
  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler

  TIM_ICStructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_PWMIConfig (Thumb, 106 bytes, Stack size 24 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TI1_Config
  - >> TI2_Config
  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler

  TIM_GetCapture1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text))
  [Called By]

  - >> TIM3_Init

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_GetITStatus (Thumb, 24 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text))
  [Called By]

  - >> TIM3_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text))
  [Called By]

  - >> TIM3_IRQHandler
  - >> TIM3_Init

  TIM_DMAConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 54 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 48 bytes, Stack size 16 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TI1_Config
  - >> TI2_Config
  - >> TIM_SelectInputTrigger

  TIM_ETRConfig (Thumb, 18 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 30 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 22 bytes, Stack size 8 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_SelectOutputTrigger (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 42 bytes, Stack size 16 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_SelectHallSensor (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  TIM_RemapConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_tim.o(.text), UNUSED)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_uidivmod
  [Called By]
  - >> RCC_GetClocksFreq
  - >> USART_Init
  - >> SystemCoreClockUpdate
  - >> delay_init
  - >> __aeabi_idivmod

  __aeabi_idiv (Thumb, 0 bytes, Stack size 16 bytes, idiv.o(.text), UNUSED)

  __aeabi_idivmod (Thumb, 40 bytes, Stack size 16 bytes, idiv.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = __aeabi_idivmod ⇒ __aeabi_uidivmod
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> displayHarmI
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayFreq
  - >> displayPData
  - >> displayHarmU
  - >> displayLC
  - >> displayMD
  - >> displayTempata
  - >> displayPowerData
  - >> displayUIData

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> USART1SendData
  - >> ExistRXInformation

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> requestData
  - >> keyHandle
  - >> ExistRXInformation

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_fmul (Thumb, 122 bytes, Stack size 16 bytes, fmul.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> displayHarmI
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayFreq
  - >> displayPData
  - >> displayHarmU
  - >> displayLC
  - >> displayMD
  - >> displayTempata
  - >> displayPowerData
  - >> displayUIData

  __aeabi_fdiv (Thumb, 124 bytes, Stack size 16 bytes, fdiv.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fdiv
  [Calls]
  - >> _float_round
  [Called By]
  - >> displayPageInformation
  - >> GetDatalength

  __aeabi_f2iz (Thumb, 50 bytes, Stack size 0 bytes, ffixi.o(.text))
  [Called By]

  - >> displayHarmI
  - >> displayPDataSpec
  - >> displayPDataSpecVA
  - >> displayFreq
  - >> displayPData
  - >> displayHarmU
  - >> displayLC
  - >> displayMD
  - >> displayTempata
  - >> displayPowerData
  - >> displayUIData

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 16 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_fdiv

  _float_epilogue (Thumb, 114 bytes, Stack size 12 bytes, fepilogue.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __ARM_common_switch8 (Thumb, 26 bytes, Stack size 8 bytes, main.o(i.__ARM_common_switch8))
  [Stack]

  - Max Depth = 8
  - Call Chain = __ARM_common_switch8
  [Called By]
  - >> displayPageInformation
  - >> displayCtnum
  - >> displayPowerData

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SetSysClock (Thumb, 198 bytes, Stack size 24 bytes, system_stm32f0xx.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SetSysClock ⇒ RCC_PLLConfig
  [Calls]
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLConfig
  [Called By]
  - >> SystemInit

  TI4_Config (Thumb, 46 bytes, Stack size 16 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI3_Config (Thumb, 44 bytes, Stack size 16 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI2_Config (Thumb, 42 bytes, Stack size 20 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 40 bytes, Stack size 16 bytes, stm32f0xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  ### Undefined Global Symbols

  __arm_fini_ (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_shutdown_fini