#

##

##

##

##

##

##

    킮ision Build Log
    Tool Versions:
    IDE-Version: ┢Vision V5.33.0.0
    Copyright (C) 2020 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: Maackia Administrator, M, LIC=EXJT4-FXNDZ-IIV5V-PIASW-PP11J-3MZ6T

    Tool Versions:
    Toolchain:       MDK-ARM Plus  Version: 5.33.0.0
    Toolchain Path:  D:\MDK5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 7 (build 960)
    Assembler:       Armasm.exe V5.06 update 7 (build 960)
    Linker/Locator:  ArmLink.exe V5.06 update 7 (build 960)
    Library Manager: ArmAr.exe V5.06 update 7 (build 960)
    Hex Converter:   FromElf.exe V5.06 update 7 (build 960)
    CPU DLL:         SARMCM3.DLL V5.33.0.0
    Dialog DLL:      DARMCM1.DLL V1.19.4.0
    Target DLL:      Segger\JL2CM3.dll V2.99.38.0
    Dialog DLL:      TARMCM1.DLL V1.14.3.0

    Project:
    D:\work\Project\F030\9.14 뙈쯤팁劤혜땡\10.16 뙈쯤팁\8.11 뙈쯤팁 - 꿎桿\User\STM32F030Demo.uvprojx
    Project File Date:  11/29/2022

    Output:
    *** Using Compiler 'V5.06 update 7 (build 960)', folder: 'D:\MDK5\ARM\ARMCC\Bin'
    Rebuild target 'Stm32f030demo'
    assembling startup_stm32f0xx.s...
    compiling system_stm32f0xx.c...
    compiling stm32f0xx_it.c...
    compiling gpio.c...
    compiling delay.c...
    compiling ht16c23.c...
    compiling main.c...
    compiling key.c...
    ..\HARDWARE\src\key.c(33): warning:  #1295-D: Deprecated declaration USART1SendData - give arg types
      extern void USART1SendData();
    ..\HARDWARE\src\key.c: 1 warning, 0 errors
    compiling myiic.c...
    compiling usart.c...
    ..\HARDWARE\src\usart.c(277): warning:  #550-D: variable "Clear"  was set but never used
      	u8 Clear;
    ..\HARDWARE\src\usart.c(368): warning:  #167-D: argument of type "volatile DataStructure *" is incompatible with parameter of type "void *restrict"
      				memcpy(&DataStruc, &rsRxBuf[6],sizeof(DataStruc));
    ..\HARDWARE\src\usart.c(356): warning:  #177-D: variable "tmp"  was declared but never referenced
      	u8 tmp[5] = {0xfa,0xfb,0xfa,0xfb,0x04};
    ..\HARDWARE\src\usart.c: 3 warnings, 0 errors
    compiling oled0561.c...
    compiling led.c...
    compiling stm32f0xx_gpio.c...
    compiling stm32f0xx_misc.c...
    compiling stm32f0xx_rcc.c...
    compiling stm32f0xx_crc.c...
    compiling stm32f0xx_usart.c...
    compiling stm32f0xx_i2c.c...
    compiling stm32f0xx_syscfg.c...
    compiling stm32f0xx_dma.c...
    compiling stm32f0xx_tim.c...
    linking...
    Program Size: Code=26060 RO-data=864 RW-data=108 ZI-data=2092
    FromELF: creating hex file...
    "..\OBJ\STM32F030Demo.axf" - 0 Error(s), 4 Warning(s).

    Software Packages used:

    Package Vendor: ARM
                    http://www.keil.com/pack/ARM.CMSIS.5.7.0.pack
                    ARM.CMSIS.5.7.0
                    CMSIS (Cortex Microcontroller Software Interface Standard)
       * Component: CORE Version: 5.4.0

    Package Vendor: Keil
                    http://www.keil.com/pack/Keil.STM32F0xx_DFP.1.4.0.pack
                    Keil.STM32F0xx_DFP.1.4.0
                    STMicroelectronics STM32F0 Series Device Support and Examples

    Collection of Component include folders:
      .\RTE\_Stm32f030demo
      D:\MDK5\ARM\PACK\ARM\CMSIS\5.7.0\CMSIS\Core\Include
      D:\MDK5\ARM\PACK\Keil\STM32F0xx_DFP\1.4.0\Device\Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:5.4.0
    Build Time Elapsed:  00:00:03